**MODULATION TRANSFER FUNCTION IN IMAGE PROCESSING**

Measures the ability of a sensor to resolve signals at different frequencies

* Frequency is measured in line pairs (lp)/mm
* Detectability is measured in %

It is calculated by,

DQE(f) = K[MTF(f)]^2 / [σ(f)]^2