**MODULATION TRANSFER FUNCTION IN IMAGE PROCESSING**

* MTF is the ability of the detector to transfer the inflection of the input signal at a given spatial frequency to its output.

**PRACTICAL CALCULATION**

* RGB conversion
* Edge detection
* Calculation of ESF, LSF and SFR